|  |  |
| --- | --- |
| Input Voltage | DC 9V-16V |
| Input Current | ≤15A |
| Output Voltage | DC 9V-16V |
| ACC Voltage | DC 9V-16V |
| Each Output Current | 3A |
| Single Output Current | ≤5A |
| MAX Output Power | ≤200W |
| Standby Current | ≤10uA |
| No Load Power Consumption | ≤0.2W |
| Waterproof IP Rating | IP67 |
| Overcurrent Protection | Fuse |
| Operating Temperature | -30℃ to 70℃ |
| Delay Output | 10 Seconds |